System should find out GPS of centers of all the photos from the flight within error no more than 100 meters in comparison to the real GPS
System should find out GPS of centers of 70% of the photos from the flight within error no more than 30 meters in comparison to the real GPS
